**LAB 4 Report**

**Name: Dhruv Sandesara**


**UT EID: djs3967**

**Section: 15295**


**Checklist:**

**Part 1 -**

1. Simulation waveform of the Flight Attendant Call System for behavioral as well as dataflow modelling



1. K-map for minimizing the expression for next\_state for dataflow modelling



1. Boolean expression for next\_state for dataflow modelling

*next\_state = call\_button | (~cancel\_button&light\_state)*

1. Completed design file (.v) for dataflow modelling

*module flight\_attendant\_call\_system\_dataflow(*

*input wire clk,*

*input wire call\_button,*

*input wire cancel\_button,*

*output reg light\_state*

*);*

*wire next\_state;*

*assign next\_state= call\_button|(~cancel\_button&light\_state);*

*always@(posedge clk) begin*

*light\_state<=next\_state;*

*end*

*endmodule*

**Part 2 -**

1. State Diagram of the Rising Edge Detector
2. Completed design files (.v) including the top module and clock divider

*module rising\_edge\_detector(*

*input clk,*

*input signal,*

*input reset,*

*output reg outedge*

*);*

*wire slow\_clk;*

*reg[1:0] state;*

*reg[1:0] next\_state;*

*clkdiv cl(clk, reset, slow\_clk);*

*always @(\*) begin*

*2'b00 : begin*

*outedge = 1'b0;*

*if(~signal)*

*next\_state = 2'b00;*

*else*

*next\_state = 2'b01;*

*end*

*2'b01 : begin*

*outedge = 1'b1;*

*next\_state = 2'b10;*

*end*

*2'b10 : begin*

*outedge = 1'b0;*

*if(~signal)*

*next\_state = 2'b00;*

*else*

*next\_state = 2'b10;*

*end*

*default : begin*

*next\_state = 2'b00;*

*outedge = 1'b0;*

*end*

*endcase*

*end*

*always @(posedge slow\_clk) begin*

*if(reset)*

*state <= 2'b00;*

*else*

*state <= next\_state;*

*end*

*endmodule*

*module clkdiv(*

*input clk,*

*input reset,*

*output clk\_out*

*);*

*reg[20:0] COUNT;*

*assign clk\_out = COUNT[20];*

*always @(posedge clk)*

*begin*

*if(reset)*

*COUNT = 0;*

*else*

*COUNT = COUNT + 1;*

*end*

*endmodule*

1. Test-bench of the system

*module tb\_rising\_edge\_detector;*

*reg clk;*

*reg signal;*

*reg reset;*

*wire outedge;*

*rising\_edge\_detector u1(*

*.clk(clk),*

*.signal(signal),*

*.reset(reset),*

*.outedge(outedge)*

*);*

*clkdiv u2(*

*.clk(clk)*

*);*

*initial*

*begin*

*clk = 0;*

*signal = 0;*

*reset = 1;*

*#10*

*signal = 0;*

*reset = 0;*

*#30*

*signal = 1;*

*reset = 0;*

*#40*

*signal = 1;*

*reset = 0;*

*#40*

*signal = 0;*

*reset = 0;*


*end*

*always*

*#5 clk = ~clk;*

*endmodule*

1. Simulation waveform



1. Constraints File (Just the uncommented portion)

set\_property PACKAGE\_PIN W5 [get\_ports clk]

set\_property IOSTANDARD LVCMOS33 [get\_ports clk]

create\_clock -add -name sys\_clk\_pin -period 10.00 -waveform {0 5} [get\_ports clk]

set\_property PACKAGE\_PIN V17 [get\_ports {signal}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {signal}]

set\_property PACKAGE\_PIN U16 [get\_ports {outedge}]

set\_property IOSTANDARD LVCMOS33 [get\_ports {outedge}]

set\_property PACKAGE\_PIN U18 [get\_ports reset]

set\_property IOSTANDARD LVCMOS33 [get\_ports reset]

**Part 3 -**

1. Completed design files (.v) of all the modules in the system

*module time\_multiplexing\_main(*

*input clk,*

*input reset,*

*input [15:0] sw,*

*output [3:0] an,*

*output [6:0] sseg);*

*wire [6:0] in0, in1, in2, in3 ;*

*wire slow\_clk;*

*hexto7segment c1 (.x(sw[3:0]), .r(in0));*

*hexto7segment c2 (.x(sw[7:4]), .r(in1));*

*hexto7segment c3 (.x(sw[11:8]), .r(in2));*

*hexto7segment c4 (.x(sw[15:12]), .r(in3));*

*clkdiv c5 (.clk(clk), .reset(reset), .slow\_clk(slow\_clk));*

*time\_mux\_state\_machine c6(*

*.clk (slow\_clk),*

*.reset (reset),*

*.in0 (in0),*

*.in1 (in1),*

*.in2 (in2),*

*.in3 (in3),*

*.an (an),*

*.sseg (sseg));*

*endmodule*

*module time\_mux\_state\_machine(*

*input clk,*

*input reset,*

*input [6:0] in0,*

*input [6:0] in1,*

*input [6:0] in2,*

*input [6:0] in3,*

*output reg [3:0] an,*

*output reg [6:0] sseg*

*);*

*reg [1:0] state;*

*reg [1:0] next\_state;*

*always @(\*) begin*

*case(state)*

*2'b00: next\_state = 2'b01;*

*2'b01: next\_state = 2'b10;*

*2'b10: next\_state = 2'b11;*

*2'b11: next\_state = 2'b00;*

*endcase*

*end*

*always @(\*) begin*

*case(state)*

*2'b00: sseg = in0;*

*2'b01: sseg = in1;*

*2'b10: sseg = in2;*

*2'b11: sseg = in3;*

*endcase*

*case(state)*

*2'b00: an = 4'b1110;*

*2'b01: an = 4'b1101;*

*2'b10: an = 4'b1011;*

*2'b11: an = 4'b0111;*

*endcase*

*end*

*always @(posedge clk or posedge reset) begin*

*if(reset)*

*state <= 2'b00;*

*else*

*state <= next\_state;*

*end*

*endmodule*

*module hexto7segment(*

*input [3:0] x,*

*output reg [6:0] r*

*);*

*always @(\*)*

*case(x)*

*4'b0000 : r = 7'b0000001;*

*4'b0001 : r = 7'b1001111;*

*4'b0010 : r = 7'b0010010;*

*4'b0011 : r = 7'b0000110;*

*4'b0100 : r = 7'b1001100;*

*4'b0101 : r = 7'b0100100;*

*4'b0110 : r = 7'b0100000;*

*4'b0111 : r = 7'b0001111;*

*4'b1000 : r = 7'b0000000;*

*4'b1001 : r = 7'b0001100;*

*4'b1010 : r = 7'b0001000;*

*4'b1011 : r = 7'b1100000;*

*4'b1100 : r = 7'b0110001;*

*4'b1101 : r = 7'b1000010;*

*4'b1110 : r = 7'b0110000;*

*4'b1111 : r = 7'b0111000; endcase*

*endmodule*

*module clkdiv(*

*input clk,*

*input reset,*

*output slow\_clk*

*);*

*reg [25:0] COUNT;*

*assign slow\_clk = COUNT[25];*

*always @(posedge clk) begin*

*if(reset)*

*COUNT = 0;*

*else*

*COUNT = COUNT + 1;*

*end*

*endmodule*

1. Test-bench of the system

*module tb\_time\_multiplexing\_main;*

*reg clk;*

*reg reset;*

*reg [15:0]sw;*

*wire [3:0] an;*

*wire [6:0] sseg;*

*time\_multiplexing\_main u1(*

*.clk(clk),*

*.reset(reset),*

*.sw(sw),*

*.an(an),*

*.sseg(sseg)*

*);*

*initial begin*

*sw = 16'h0000;*

*clk = 0;*

*reset = 0;*

*#30*

*reset = 0;*

*sw = 16'h0008;*

*#30;*

*reset = 0;*

*sw = 16'h4321;*

*#30;*

*reset = 0;*

*sw = 16'h0002;*

*#30;*

*reset = 0;*

*sw = 16'h0302;*


*end*

*always*

*#5 clk = ~clk;*

*Endmodule*

1. Simulation waveform



1. Constraints File (Just the uncommented portion)

*set\_property PACKAGE\_PIN W5 [get\_ports {clk}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {clk}]*

*create\_clock -add -name sys\_clk\_pin -period 10.00 -waveform {0 5} [get\_ports {clk}]*

*set\_property PACKAGE\_PIN V17 [get\_ports {sw[0]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[0]}]*

*set\_property PACKAGE\_PIN V16 [get\_ports {sw[1]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[1]}]*

*set\_property PACKAGE\_PIN W16 [get\_ports {sw[2]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[2]}]*

*set\_property PACKAGE\_PIN W17 [get\_ports {sw[3]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[3]}]*

*set\_property PACKAGE\_PIN W15 [get\_ports {sw[4]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[4]}]*

*set\_property PACKAGE\_PIN V15 [get\_ports {sw[5]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[5]}]*

*set\_property PACKAGE\_PIN W14 [get\_ports {sw[6]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[6]}]*

*set\_property PACKAGE\_PIN W13 [get\_ports {sw[7]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[7]}]*

*set\_property PACKAGE\_PIN V2 [get\_ports {sw[8]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[8]}]*

*set\_property PACKAGE\_PIN T3 [get\_ports {sw[9]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[9]}]*

*set\_property PACKAGE\_PIN T2 [get\_ports {sw[10]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[10]}]*

*set\_property PACKAGE\_PIN R3 [get\_ports {sw[11]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[11]}]*

*set\_property PACKAGE\_PIN W2 [get\_ports {sw[12]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[12]}]*

*set\_property PACKAGE\_PIN U1 [get\_ports {sw[13]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[13]}]*

*set\_property PACKAGE\_PIN T1 [get\_ports {sw[14]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[14]}]*

*set\_property PACKAGE\_PIN R2 [get\_ports {sw[15]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sw[15]}]*

*set\_property PACKAGE\_PIN W7 [get\_ports {sseg[6]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[6]}]*

*set\_property PACKAGE\_PIN W6 [get\_ports {sseg[5]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[5]}]*

*set\_property PACKAGE\_PIN U8 [get\_ports {sseg[4]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[4]}]*

*set\_property PACKAGE\_PIN V8 [get\_ports {sseg[3]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[3]}]*

*set\_property PACKAGE\_PIN U5 [get\_ports {sseg[2]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[2]}]*

*set\_property PACKAGE\_PIN V5 [get\_ports {sseg[1]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[1]}]*

*set\_property PACKAGE\_PIN U7 [get\_ports {sseg[0]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {sseg[0]}]*

*set\_property PACKAGE\_PIN U2 [get\_ports {an[0]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {an[0]}]*

*set\_property PACKAGE\_PIN U4 [get\_ports {an[1]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {an[1]}]*

*set\_property PACKAGE\_PIN V4 [get\_ports {an[2]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {an[2]}]*

*set\_property PACKAGE\_PIN W4 [get\_ports {an[3]}]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports {an[3]}]*

*set\_property PACKAGE\_PIN U18 [get\_ports reset]*

*set\_property IOSTANDARD LVCMOS33 [get\_ports reset]*

***Note*** *🡪 The Verilog codes and the uncommented portions of the constraint files should be copied in your lab report and the* ***actual Verilog (.v), Constraint (.xdc) files and Bitstream (.bit) files*** *need to be zipped and submitted as well on Canvas. You are not allowed to change your codes after final submission as the TAs may download the submitted codes or bitstream files from Canvas during checkouts. For the truth Table, K-maps minimizations and algebraic expressions, you are free to draw them on paper and then put the pictures in your lab report, but please make sure it is legible for the TAs to grade it properly.*